**List of 30t/24h maize milling machine**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item** | **Picture** | **Product desription** | **Quantity** | **Power (kW)** | |
| **Unit** | **Total** |
|  | 斗式提升机 | Name: Bucket elevator  Type: DTG20/11  Output:2-3t/h  Dimension: 800×260×7000  Power:1.1kW | 4 | 1.1 | 4.4 |
|  | 高效筛 | Name: High efficiency vibrating sieve  Type: TQLZ60×100  Output:2-3T/H  Power: 0.25KW×2  Dimension: 1695×1175×1455  Weight:360kg | 1 | 0.25\*2 | 0.5 |
|  | 比重分级去石机 | Name: Gravity classify stoner  Type:TQSF60  Output:2-3t/h  Power: 0.25×2=0.5kw  Dimension: 1450×880×1800  Weight:280kg | 1 | 0.25\*2 | 0.5 |
|  | 着水机 | **Name:** Regulate moisture damper  Type: ZSQ3A  Output: 2-3 T/H  Power:1.1kw  Dimension: 1400×350×1050  Weight:140kg | 1 | 1.1 | 1.1 |
|  | Q7[M73R0Q_]L@FUP)PL75AC | Mid-container | 1 | 0 | 0 |
|  | **3** | Name: Low pressure blower  Type: 4-72-3.6A  Power: 3kw  Wind power: 2664-5268m3/h  Wind pressure:989-1578Pa  Dimension:610×590×720  Weight:78kg | 2 | 3 | 6 |
|  | C:\Documents and Settings\Administrator\Application Data\Tencent\Users\1070707004\QQ\WinTemp\RichOle\}~UV8{Q4{5H}C4}FGXWA7}F.png | Name: crasher  Type: 6NF-15.8  Output: 2-3t/h  Dimension: 1320×900×1450  Power:22KW  Weight:620kg | 1 | 22 | 22 |
|  |  | Name:Hammer mill  Type:SFSP56/40  Output:2-3t/h  Power:37kW  Dimension: 1650×1050×1080  Weight: 900kg | 1 | 37 | 37 |
|  |  | Name: Magnetic separator  Type: TCXT5  Output: 3~5 T/H | 2 | 0 | 0 |
|  | 2250单式磨机.jpg | Name: Roller mill  Type: 6F2250  Power:11kW  Dimension: 1200×750×1600  Weight:650kg | 1 | 11 | 11 |
|  | 83双仓筛 | **Name:**Double sifter series  Type：FSFJ2×83  Power: 1.5kw  Dimension:2122×1567×2037  Weight:980kg | 1 | 1.5 | 1.5 |
|  | 高压风机 | Name: High pressure blower  Type:TFD630-5.5#  Power:7.5kW  Wind power: 3126-5905 m3/H  Wind pressure:4135-5282Pa  Dimension: 800×620×1000  Weight:140kg | 1 | 7.5 | 7.5 |
|  | 螺旋输送机 | **Name:** Screw Conveyer  Type：LSS16  Output:1.5-3T/H  Power: 1.1KW  Weight:180kg | 1 | 1.1 | 1.1 |
|  | GFY4关风器(小) | Name: Air seal  Type：TGFY-4L  Weight:35kg | 4 | 0 | 0 |
|  |  | Name: Air seal and frank  Type: TGFY-4L  Power: 0.75kw | 1 | 0.75 | 0.75 |
|  | 减速机 | Name: Motor for air seal Reducer  Type: XWD1.1-3-29  Dimension: 480×250×230  Power:1.5kw | 1 | 1.1 | 1.1 |
|  |  | Collectors four machine | 2set | 0 | 0 |
|  |  | Name: Step-down start the ark  40KW | 1set | 0 | 0 |
|  | 电柜1 | Name: Central control panel  Dimension: 900×400×2000  Weight:100kg | 1set | 0 | 0 |
|  | P1040970.JPG | Pipes | 1 set | 0 | 0 |
|  | P1080501.JPG | Platform & support | 1 set | 0 | 0 |
|  | 手提缝口机.jpg | Name: Mobile sealing machine  Type: GK9-8  Power: 0.12KW  Dimension: 350×220×400  Weight:5kg | 1 | 0.12 | 0.12 |
|  |  | Name: digital balance scale  Voltage:AC 220V  150KG | 1set | 0 | 0 |
|  |  | Standard parts | 1set | 0 | 0 |
|  |  | Accessory | 1set | 0 | 0 |
|  |  | Cushion | 1set | 0 | 0 |
|  |  | Cables | 1set | 0 | 0 |
|  |  | Spare part one year | 1set | 0 | 0 |
|  |  | Total power |  |  | 94.57 |

**Option part: Auto packing machine**

**]**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item** | **Picture** | **Product description** | **Quantity** | **Power(kW)** | |
| **Unit** | **Total** |
|  |  | Name: Bucket elevator  Type: DTG20/11  Output:1.5-2t/h  Dimension: 8200×320×500  Weight:280kg | 1 | 1.1 | 1.1 |
|  |  | Name: Auto-weighting& packing  Type: Link-ZF25  Output: 200-240bags /H  Power: 3.15kw  Dimension:800×1060×2790mm  Weight: 650kg | 1 | 3.15 | 3.15 |
|  | 空压机3 | Name: Compressor  Type: ZW0.25/8  Power:2.2kw  Dimension: 1140×480×900  Weight:150kg | 1set | 2.2 | 2.2 |

**Technical Data**

1. Production capacity: 30t maize/24h

2. Workshop（L×W×H）：20×8×5.5m

3. Power supply: About 95kW